{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":26,"n_cols":6,"rows_kept":26,"merged":[[0,0,0,5],[2,0,2,2],[2,3,2,5],[3,3,3,4],[21,0,21,4],[22,0,22,5],[24,0,24,4]],"flags":["formulas_cached_only"]}
["二次供水水质常规分析报告表"]
[]
["送样日期：2021.3.31             送样人：苏文威",null,null,"      样品名称:碧桂园酒店水样"]
["编号","分析项目","GB5749-2006要求","检测结果",null,"结果评价"]
[1,"pH","不小于6.5且不大于8.5",{"v":7.9,"d":"7.90"},null,"合格"]
[2,"浑浊度","≤1NTU（水源与净水技术条件限制时为3NTU）",{"v":0.1,"d":"0.10"},"NTU","合格"]
[3,"色度","≤15（铂钴色度单位）","<5","度","合格"]
[4,"嗅和味","无异臭、异味",0,null,"合格"]
[5,"肉眼可见物","无","无",null,"合格"]
[6,"亚硝酸盐氮","0.3mg/L","<0.001","mg/L","合格"]
[7,"氨氮","≤0.5mg/L","<0.02","mg/L","合格"]
[8,"耗氧量","≤3.0mg/L",0.56,"mg/L","合格"]
[9,"游离余氯","出厂水≥0.3mg/L，管网末梢水≥0.05mg/L",0.25,"mg/L","合格"]
[10,"菌落总数","100(CFU/mL)","未检出","CFU/mL","合格"]
[11,"总大肠菌群","每100mL水样中不得检出","未检出","CFU/100mL","合格"]
[12,"耐热大肠菌群","每100mL水样中不得检出","未检出","CFU/100mL","合格"]
[13,"大肠埃希氏菌","每100mL水样中不得检出","未检出","MPN/100mL","合格"]
[null,"根据GB5749-2006《生活饮用水卫生标准》，检测结果符合标准要求。"]
["检测"]
["结论"]
[]
["检测依据：GB/T5750-2006"]
["审核：梅喜雪        检验者:  黄剑青  、李英姿  、李夏阳         日期：2021.4.2"]
[]
[]
[{"$nulls":3},"               台山市自来水有限公司中心化验室"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}