{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["Sheet3","Sheet1"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet3","index":0,"n_rows":18,"n_cols":6,"rows_kept":18,"merged":[[0,0,0,5],[17,0,17,4]],"flags":["formulas_cached_only"]}
["2025年台山市工业产品质量监督抽查计划"]
["序号","一级分类\n名称","二级分类\n名称","产品名称","检验项目","批次"]
[1,"日用及纺织品","文体用品","学生用品","外观（整体、封面、封面正常闭合时的张开度）、功能（转折处的耐折次数、耐温性、装订性能、夹具开合、快劳夹直立强度（刚度））",2]
[2,"日用及纺织品","儿童用品","玩具","邻苯二甲酸二丁酯（DBP）、邻苯二甲酸丁苄酯(BBP)、\n邻苯二甲酸二（2-乙基）己酯(DEHP)",1]
[3,"日用及纺织品","纺织品","校服","甲醛含量、可分解致癌芳香胺染料、耐水色牢度、绳带要求",1]
[4,"日用及纺织品","日用杂品","塑料垃圾袋","厚度及偏差、有效宽度偏差、有效长度偏差、抗渗漏性能、跌落性能、提吊试验",5]
[5,"机械及安防","车辆及相关产品","电动自行车头盔","耐刺穿性性能、头盔视野",6]
[6,"机械及安防","车辆及相关产品","车用汽油","研究法辛烷值、硫含量、苯含量、芳烃含量",1]
[7,"机械及安防","车辆及相关产品","电动自行车电池","容量、大电流放电",1]
[8,"机械及安防","安全技术防范产品","危险化学品包装物","液压性能、跌落试验、堆码试验",5]
[9,"电工及材料","电线及电\n缆","电线电缆","导体电阻、绝缘平均厚度、绝缘最薄处厚度、护套平均厚度、护套最薄处厚度、绝缘老化前抗张强度、绝缘老化前断裂伸长率",2]
[10,"轻工产品","燃气用具","家用燃气灶","气密性、热负荷偏差、离焰、熄火、回火、干烟气中一氧化碳浓度、温升、操作时手必需接触部位）、耐热冲击、耐重力冲击、熄火保护、装置\n热效率、燃气导管",1]
[11,"轻工产品","眼镜类产\n品","老年眼镜","镜片表面质量和内在疵病、镜架外观质量、球镜顶焦度偏差、光学中心水平距离偏差、光学中心垂直互差、装配质量、标志",5]
[12,"轻工产品","纸及制品","瓦楞纸箱","耐破强度、粘合强度、抗压强度",5]
[13,"轻工产品","化工产品","危险化学品（溶剂型涂料）","VOC含量、苯含量、甲苯与二甲苯（含乙苯）含量总和",1]
[14,"建筑和装饰装修材料","建筑钢材","热轧带肋钢筋","力学性能（屈服强度、抗拉强度、断后伸长率、实测抗拉强度与实测屈服强度之比、实测屈服强度与屈服强度特征值之比、最大力总延伸率）、工艺性能（弯曲、反向弯曲）、化学成分（C、Si、Mn、P、S、Ceq）、尺寸外形（横肋高、肋间距、横肋末端最大间隙、每米弯曲度）、重量偏差、金相组织、表面标志",5]
[15,"建筑和装饰装修材料","新型墙体材料","新型墙体材料","强度等级、石灰爆裂、抗风化性能、泛霜 、密度等级、孔型孔结构及孔洞率、放射性",5]
["合计：",{"$nulls":4},46]

{"sheet":"Sheet1","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}